# SUPPORTED UMAX SCANNERS

> The sane-umax library implements a SANE backend that provides acces to several UMAX-SCSI-scanners. Parallel- and USB- scanners are not supported!
> Here is a list of the UMAX-scanners:

UMAX scanners
Vista series: (also see at the table old UMAX scanners)
Name | SCSI-ID | Versions | UTA | ADF | Lineart | Grayscale | Color RGB | Bits/pixel | Optical resolution
Vista S6 | Vista-S6 | all | X | X | ok | ok | ok | 1,8,24 | 300 x 600
Vista S6E | Vista-S6E | all | X | X | ok | ok | ok | 1,8,24 | 300 x 600
Vista S6E | UMAX S-6E | all | X | X | ok | ok | ok | 1,8,24 | 300 x 600
Vista S6E | UMAX S-6EG | all | X | X | ok | ok | ok | 1,8,24 | 300 x 600
Vista S8 | Vista-S8 | all | X | X | ok | ok | ok | 1,8,24 | 400 x 800
Supervista S12 | Supervista S-12 | all | X | X | ok | ok | ok | 1,8,24 | 600 x 1200*
Supervista S12 | UMAX S-12G | all | X | X | ok | ok | ok | 1,8,24 | 600 x 1200*
Supervista S12 | UMAX S-12 | all | X | X | ok | ok | ok | 1,8,24 | 600 x 1200*
Astra series:
Name | SCSI-ID | Versions | UTA | ADF | Lineart | Grayscale | Color RGB | Bits/pixel | Optical resolution
Astra 600S | Astra 600S | all | X |  | ok | ok | ok | 1,8,24 | 300 x 600
Astra 610S | Astra 610S | all | -- |  | ok | ok | ok | 1,8,24 | 300 x 600
Astra 1200S | Astra 1200S | all but 2.9 *** | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
Astra 1220S | Astra 1220S | all | X |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Astra 2200W | Astra 2200 | all (2.1) **** | X |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Astra 2400S | Astra 2400S | all (1.1) | X | X | ok | ok | ok | 1,8,12,24,36 | 600 x 2400
Mirage series:
Name | SCSI-ID | Versions | UTA | ADF | Lineart | Grayscale | Color RGB | Bits/pixel | Optical resolution
Mirage | Mirage D-16L | all (2.7) | incl |  | ok | ok | ok | 1,8,10,24,30 | 400 x 800 800 x 1600**
Mirage II | Mirage II | ? | incl |  | ? | ? | ? | 1,8,12,24,36 | 700 x 1400 1400 x 2800
Mirage IIse | Mirage IIse | ? | incl |  | ? | ? | ? | 1,8,12,24,36 | 700 x 1400
Power Look series:
Name | SCSI-ID | Versions | UTA | ADF | Lineart | Grayscale | Color RGB | Bits/pixel | Optical resolution
PowerLook | unknown | ? | X |  | ? | ? | ? | 1,8,10,24,30 | 600 x 1200
PowerLook II | PL-II | ? | X |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Power Look III | Power Look III | ? | X |  | ? | ? | ? | 1,8,14,24,42 | 1200 x 2400
PowerLook 2000 | Power Look 2000 | ? | incl |  | ? | ? | ? | 1,8,12,24,36 | 1000 x 2000
PowerLook 3000 | Power Look 3000 | ? | incl |  | ? | ? | ? | 1,8,14,24,42 | 1220 x 3048 3048 x 3048
PowerLook 1600XL | unknown | ? | incl |  | ? | ? | ? | 1,8,14,24,42 | 800 x 1600
Other scanners:
Name | SCSI-ID | Versions | UTA | ADF | Lineart | Grayscale | Color RGB | Bits/pixel | Optical resolution
Gemini D-16 | Gemini D-16 | ? | X |  | ok | ok | ok | 1,8,10,24,30 | 400 x 800 800 x 1600
PageScan | PSD | all | -- |  | ok | ok | ok | 1,8,24 | 300 x 300

* Supervista S12 scanners allow scanning up to 1200x1200 dpi.
** Mirage D-16L scanners allow scanning up to 800x800 / 1600x1600 dpi.
*** Astra 1200S-C with external power supply and Firmware Version 2.9 could make problems.
**** Astra 2200W is supported via SCSI. Connection via the USB bus not tested.

UTA = Umax Transparancy Adapter, ADF = Automatic Document Feeder
(X = supported by scanner, incl = is included)

SANE-UMAX index

This page has been changed on 5th. january 2000