NetWare for SAA 1.3 Rev. A Installation Summary
                   for NetWare 3.12


  The installation procedures in this installation ReadMe file
describe how to install NetWare for SAA 1.3 Rev. A to a local 
server. 


                        Is NetWare 3.12
                     running on the server?

            YES                                         NO

  Backup the server if necessary.               Install NetWare 3.12.
                                                See the NetWare 3.12
                                                Installation Guide.



EDITING THE AUTOEXEC.NCF FILE

1.  Start the server on which you are going to install NetWare for
    SAA 1.3 Rev. A.

2.  Enter this command: LOAD INSTALL <Enter>.

3.  Select System Options from the Installation menu.

4.  Select the Edit AUTOEXEC.NCF option; then add the following 
    commands BEFORE the commands that load the LAN drivers.

    LOAD CLIB
    LOAD BTRIEVE -U=1 -P=4096 -F=20 -H=60 -L=20 -C
    SET MAXIMUM PACKET RECEIVE BUFFERS=2000

5.  Press <Esc>; then save the changes in the file.


LOADING THE BTRIEVE NLM

  Load the BTRIEVE NLM at the system console with the following 
parameters:

    LOAD BTRIEVE -U=1 -P=4096 -F=20 -H=60 -L=20 -C


DECIDING WHERE TO INSTALL NETWARE FOR SAA 1.3 REV. A

  You can install NetWare for SAA from diskettes, from a DOS 
partition, or a from NetWare partition.

    NOTE: Installing from diskettes may take up to four times
    longer to complete.


INSTALLING NETWARE FOR SAA FROM DISKETTES

1.  At the server console prompt ( : ), type LOAD INSTALL <Enter>.

2.  Select Product Options and press <Enter>.

3.  To install the Communication Executive, press <Insert>. Then 
    insert NetWare for SAA COMMEXEC Disk 1 into Drive A: and press 
    <Enter>.

4.  Select "Install on this server."

5.  Continue to insert diskettes as prompted until the 
    Communication Executive is installed.

6.  When the Communication Executive installation is completed,    
    press <Esc> to return to the Currently Installed Products screen.

7.  To install NetWare for SAA, press <Insert>. Then insert the 
    NetWare for SAA Installation Disk 1 into Drive A: and press 
    <Enter>. 

8.  Select "Install on this server."     

9.  Insert the NetWare for SAA License diskette as prompted and 
    press <Enter>.

10. Continue to insert diskettes as prompted until NetWare for    
    SAA 1.3 Rev. A is installed.

11. When the Communication Executive and NetWare for SAA 1.3 
    Rev. A are installed, press <Esc> to return to the Currently 
    Installed Products screen.

12. Go to "FINISHING THE INSTALLATION PROCEDURE" at the end of
    this ReadMe file.


INSTALLING NETWARE FOR SAA FROM A DOS PARTITION

    NOTE: To install NetWare for SAA 1.3 Rev. A from a DOS 
    partition, you need a minimum of 10 MB of free DOS disk 
    space as a temporary holding area for your source 
    installation files.

1.  If the server on which you intend to install NetWare for SAA 
    is running, bring down the server (with the DOWN command), 
    then type EXIT to return to DOS.

2.  Create a subdirectory called CE13 in your DOS partition.

3.  Insert the NetWare for SAA COMMEXEC Disk 1 into the floppy    
    drive; then copy the files to the Communication Executive     
    subdirectory. For example, for your C: drive, enter:

        XCOPY A:*.* C:[pathname]\CE13\*.* /s /v <Enter>

    Repeat the copy operation for each COMMEXEC installation 
    diskette.

4.  Create a subdirectory called NWSAA13.

5.  Insert the NetWare for SAA Installation Disk 1 into the floppy    
    drive; then copy the files to the NetWare for SAA subdirectory.    
    For example, for your C: drive, enter:

        XCOPY A:*.* C:[pathname]\NWSAA13\*.* /s /v

    Repeat the copy operation for each NetWare for SAA installation     
    diskette. 

6.  To restart the server, enter the following command: 

        SERVER <Enter>

7.  At the server console prompt ( : ), enter the following command:

        LOAD INSTALL <Enter>

8.  Select Product Options and press <Enter>.

9.  To install the Communication Executive, press <Insert>. Enter 
    the full pathname to the Communication Executive subdirectory
    on the DOS partition. For example:

        C:[pathname]\CE13 <Enter>

10. Select "Install on this server."

11. When the Communication Executive installation is completed,    
    press <Esc> to return to the Currently Installed Products screen.

12. To install NetWare for SAA, press <Insert>. Enter the full 
    pathname to the NetWare for SAA subdirectory on the DOS 
    partition. For example:

                C:[pathname]\NWSAA13 <Enter>

13. Select "Install on this server."

14. Insert the NetWare for SAA License diskette as prompted and     
    press <Enter>.

15. When the Communication Executive and NetWare for SAA 1.3 Rev. 
    A are installed, press <Esc> to return to the Currently 
    Installed Products screen.

16. Go to "FINISHING THE INSTALLATION PROCEDURE" at the end of
    this ReadMe file.



INSTALLING NETWARE FOR SAA FROM A NETWARE PARTITION

1.  Log in from a workstation to the server on which you are going    
    to install NetWare for SAA 1.3 Rev. A.

2.  Create the following two subdirectories under the root in the 
    SYS: volume:

        SYS:CE13
        SYS:NWSAA13

3.  Insert the NetWare for SAA COMMEXEC Disk 1 into the floppy    
    drive; then copy the files to the Communication Executive     
    subdirectory. For example:

        NCOPY A:*.* [drive]:SYS:CE13 /s <Enter>

    Repeat the copy operation for each COMMEXEC installation 
    diskette.

4.  Insert the NetWare for SAA Installation Disk 1 into the floppy    
    drive; then copy the files to the NetWare for SAA subdirectory.     
    For example:

        NCOPY A:*.* [drive]:SYS:NWSAA13 /s <Enter>

    Repeat the copy operation for each NetWare for SAA installation      
    diskette.

5.  At the server console prompt ( : ), enter the following command:

        LOAD INSTALL <Enter>

6.  Select Product Options and press <Enter>.

7.  To install the Communication Executive, press <Insert>. Enter 
    the full pathname to the Communication Executive subdirectory 
    on your SYS: volume. For example:

        SYS:CE13 <Enter>

8.  Select "Install on this server."

9.  When the Communication Executive installation is completed,    
    press <Esc> to return to the Currently Installed Products screen.

10. To install NetWare for SAA, press <Insert>. Enter the full    
    pathname to the NetWare for SAA subdirectory on your SYS:      
    volume. For example:

        SYS:NWSAA13 <Enter>

11. Select "Install on this server."

12. Insert the NetWare for SAA License diskette as prompted and     
    press <Enter>.

13. When the Communication Executive and NetWare for SAA 1.3 
    Rev. A are installed, press <Esc> to return to the Currently 
    Installed Products screen.


FINISHING THE INSTALLATION PROCEDURE

1.  To return to the server console prompt ( : ), press <Esc>.

2.  Run the DOWN command to down the server; then type EXIT to 
    return to DOS.

3.  At the DOS prompt, run the SERVER command.



    Verify that the server comes up without any error messages.    
When the server is running, you are ready to configure the SAA 
service profiles.





[Filename:312A_RM.TXT   7/29/93]
